;d##OTHER##;DN##LENGTH##MILLIMETERS;PN##PIPING_PRESSURE##PASCALS;Connection Type##OTHER##;Item_descripton##OTHER##;Catalog_code##OTHER##;Weight##PIPE_MASS##KILOGRAMS;Valve Operation##OTHER##;Valve Mechanism##OTHER##;URL##OTHER##;Type_index##OTHER##;Titolo Omniclass##OTHER##;Stem Material##OTHER##;Shaft Material##OTHER##;Rb##LENGTH##MILLIMETERS;Rq##LENGTH##MILLIMETERS;R8##LENGTH##MILLIMETERS;R7##LENGTH##MILLIMETERS;R6##LENGTH##MILLIMETERS;R5##LENGTH##MILLIMETERS;R4##LENGTH##MILLIMETERS;R3##LENGTH##MILLIMETERS;R2##LENGTH##MILLIMETERS;R1##LENGTH##MILLIMETERS;Produttore##OTHER##;PN Rating##OTHER##;Overall Width##LENGTH##MILLIMETERS;Overall Length##LENGTH##MILLIMETERS;Overall Height##LENGTH##MILLIMETERS;O-Ring Material##OTHER##;Numero Omniclass##OTHER##;Modello##OTHER##;Material##OTHER##;Manufacturers Telephone Number##OTHER##;Manufacturers Email##OTHER##;Manufacturers Address##OTHER##;Z##LENGTH##MILLIMETERS;Prospetto di default##LENGTH##MILLIMETERS;L6##LENGTH##MILLIMETERS;L5##LENGTH##MILLIMETERS;L2##LENGTH##MILLIMETERS;L4##LENGTH##MILLIMETERS;L3##LENGTH##MILLIMETERS;L1##LENGTH##MILLIMETERS;L##LENGTH##MILLIMETERS;IfcDescription##OTHER##;Hs##LENGTH##MILLIMETERS;H3##LENGTH##MILLIMETERS;H2##LENGTH##MILLIMETERS;H1##LENGTH##MILLIMETERS;H Handle##LENGTH##MILLIMETERS;General##OTHER##;Female plain ends##OTHER##;Famiglia e tipo##OTHER##;Famiglia##OTHER##;F##LENGTH##MILLIMETERS;Estrusione5##OTHER##;Estrusione4##OTHER##;Estrusione3##OTHER##;Estrusione2##OTHER##;Estrusione1##OTHER##;E##LENGTH##MILLIMETERS;Df##LENGTH##MILLIMETERS;D2##LENGTH##MILLIMETERS;D1##LENGTH##MILLIMETERS;D##LENGTH##MILLIMETERS;C2##LENGTH##MILLIMETERS;C1##LENGTH##MILLIMETERS;B##LENGTH##MILLIMETERS;Double ends##OTHER##;Dimensioni##OTHER##;Dimensione totale##OTHER##;Descrizione##OTHER##;Commenti sul tipo##OTHER##;Codice assieme##OTHER##;Closer Material##OTHER##;Classification Value##OTHER##;Classification Name##OTHER##;CE Mark##OTHER##;Q##LENGTH##MILLIMETERS;Bushes Material##OTHER##;Body Material##OTHER##;A##LENGTH##MILLIMETERS
FDRPFH0750;"75 (2""""1/2)";65;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN65;FDRPFH0750;1,656;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;65;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;67;30,5;9,5;15;72,5;12,64150943;37,96033994;42,94871795;52,96442688;58,26086957;Polypipe Italia s.r.l.;PN10;134;302,5;275;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;48;51,17511025;100,0343336;30,5106383;32;65,04854369;50;100;20;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;15;63;132;80;29;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN65;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;28,5106383;0;0;0;0;1;34,01015228;185;107,0425532;114,0425532;25;113;246;134;1;65 mmø-65 mmø;65 mmø-65 mmø;"Butterfly Valve PROFLOW H PVC-U, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.75-2""1/2";;FDRPFH0750;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;61;PVC-U;PVC-U;50
FDRPFH0900;"90 (3"""")";80;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN80;FDRPFH0900;1,856;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;80;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;69,5;36,5;9,5;15;80;13,11320755;39,37677054;44,55128205;54,94071146;60,43478261;Polypipe Italia s.r.l.;PN10;139;302,5;287;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;59;51,17511025;100,0343336;31,57446809;38;67,47572816;51,86567164;106,8827715;20;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;15;63;132;92;29;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN80;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;29,57446809;0;0;0;1;0;35,27918782;200;123;130;25;113;246;139;1;80 mmø-80 mmø;80 mmø-80 mmø;"Butterfly Valve PROFLOW H PVC-U, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.90-3""";;FDRPFH0900;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;73;PVC-U;PVC-U;50
FDRPFH1100;"110 (4"""")";100;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN100;FDRPFH1100;2,137;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;100;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;75;41;9,5;16,09135024;90;14,1509434;42,49291785;48,07692308;59,28853755;65,2173913;Polypipe Italia s.r.l.;PN10;150;302,5;301;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;59,5;51,17511025;100;33,91489362;61,47540984;72,81553398;55,97014925;104;20;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;15;63;132;106;29;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN100;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;31,91489362;0;0;1;0;0;38,07106599;220;143;150;25;113;246;150;1;100 mmø-100 mmø;100 mmø-100 mmø;"Butterfly Valve PROFLOW H PVC-U, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.110-4""";;FDRPFH1100;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;82;PVC-U;PVC-U;50
FDRPFH1400;"125/140 (5"""")";125;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN125;FDRPFH1400;2,974;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;125;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;92,5;53,5;9,5;16,09135024;105;17,45283019;52,40793201;59,29487179;73,12252964;80,43478261;Polypipe Italia s.r.l.;PN10;185;302,5;341;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;65;51,17511025;100,0343336;41,36170213;75,81967213;89,80582524;69,02985075;120;20;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;15;63;159;119;29;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN125;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;39,36170213;0;0;1;0;0;46,95431472;250;178;185;25;113;246;185;1;125 mmø-125 mmø;125 mmø-125 mmø;"Butterfly Valve PROFLOW H PVC-U, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.125/140-5""";;FDRPFH1400;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;107;PVC-U;PVC-U;50
FDRPFH1600;"160 (6"""")";150;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN150;FDRPFH1600;4,922;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;150;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;105;64;12;16,09135024;120;19,81132075;59,49008499;67,30769231;83,00395257;91,30434783;Polypipe Italia s.r.l.;PN10;210;470;428;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;69;51,17511025;100,0343336;46,68085106;86,06557377;101,9417476;78,35820896;129;20;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;20;83;215;130;40;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN150;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;44,68085106;0;0;1;0;0;53,29949239;285;203;210;30,97345133;140;400;210;1;150 mmø-150 mmø;150 mmø-150 mmø;"Butterfly Valve PROFLOW H PVC-U, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.160-6""";;FDRPFH1600;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;128;PVC-U;PVC-U;61,94690265
FDRPFH2250;"200/225 (8"""")";200;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN200;FDRPFH2250;4,968;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;200;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;134,5;88,5;12;16,09135024;147,5;25,37735849;76,20396601;86,21794872;106,3241107;116,9565217;Polypipe Italia s.r.l.;PN10;269;470;458;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;71;51,17511025;100,0343336;59,23404255;110,2459016;130,5825243;100,3731343;155;20;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;20;83;215;160;40;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast:DN200;PVC-U Butterfly valve PROFLOW H serie, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges _Effast;57,23404255;0;0;1;0;0;68,27411168;340;262;269;30,97345133;140;400;269;1;200 mmø-200 mmø;200 mmø-200 mmø;"Butterfly Valve PROFLOW H PVC-U, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.200/225-8""";;FDRPFH2250;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;177;PVC-U;PVC-U;61,94690265
FDRPFH1600.F;"160 (6"""")";150;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast:DN150;FDRPFH1600.F;4,922;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;150;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;105;64;12;16,09135024;120;19,81132075;59,49008499;67,30769231;83,00395257;91,30434783;Polypipe Italia s.r.l.;PN10;210;470;428;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;69;51,17511025;100,0343336;46,68085106;86,06557377;101,9417476;78,35820896;129;20;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast;20;83;215;130;40;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast:DN150;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast;44,68085106;0;1;0;0;0;53,29949239;285;203;210;30,97345133;140;400;210;1;150 mmø-150 mmø;150 mmø-150 mmø;"Butterfly Valve PROFLOW H PVC-U, full drilled version, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.160-6""";;FDRPFH1600.F;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;128;PVC-U;PVC-U;61,94690265
FDRPFH2250.F;"200/225 (8"""")";200;10;Installation between EN/ISO/DIN, ANSI and JIS flanges;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast:DN200;FDRPFH2250.F;4,968;Handle;HighFlow disc;https://www.effast.com/it/prodotto/pvc-u-valvola-a-farfalla-proflow-h-2/;200;Adjusting/Controlling Valves for Liquid Services;Zinc Plated Carbon Steel;PVC-U;134,5;88,5;12;16,09135024;147,5;25,37735849;76,20396601;86,21794872;106,3241107;116,9565217;Polypipe Italia s.r.l.;PN10;269;470;458;EPDM;23.65.55.14.17;Butterfly Valve type PROFLOW H Serie PVC-U;PVC-U;39018592399;info@effast.com;Loc. Pianmercato 5 16044 Cicagna (GE) Italy;71;51,17511025;100,0343336;59,23404255;110,2459016;130,5825243;100,3731343;155;20;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast;20;83;215;160;40;Bureau Veritas Mark, CE Mark, NSF Mark;0;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast:DN200;PVC-U Butterfly valve PROFLOW H serie, full drilled version Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges_Effast;57,23404255;1;0;0;0;0;68,27411168;340;262;269;30,97345133;140;400;269;1;200 mmø-200 mmø;200 mmø-200 mmø;"Butterfly Valve PROFLOW H PVC-U, full drilled version, Zinc Plated Carbon Steel Stem - Installation between EN/ISO/DIN, ANSI and JIS flanges - d.200/225-8""";;FDRPFH2250.F;PVC-U;Pr_65_54_95_08;Uniclass2015;Yes;177;PVC-U;PVC-U;61,94690265
